FQBN: arduino:avr:uno

Using board 'uno' from platform in folder: C:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6

Using core 'arduino' from platform in folder: C:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6

Detecting libraries used...

C:\Users\howar\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7/bin/avr-g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -flto -w -x c++ -E -CC -mmcu=atmega328p -DF\_CPU=16000000L -DARDUINO=10607 -DARDUINO\_AVR\_UNO -DARDUINO\_ARCH\_AVR -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\cores\arduino -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\variants\standard C:\Users\howar\AppData\Local\Temp\arduino\sketches\F46E52024E025C3DF34C17E974EB4F88\sketch\petitcat\_arduino.ino.cpp -o nul

Alternatives for Arduino\_JSON.h: [Arduino\_JSON@0.2.0]

ResolveLibrary(Arduino\_JSON.h)

-> candidates: [Arduino\_JSON@0.2.0]

C:\Users\howar\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7/bin/avr-g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -flto -w -x c++ -E -CC -mmcu=atmega328p -DF\_CPU=16000000L -DARDUINO=10607 -DARDUINO\_AVR\_UNO -DARDUINO\_ARCH\_AVR -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\cores\arduino -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\variants\standard -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino\_JSON\src C:\Users\howar\AppData\Local\Temp\arduino\sketches\F46E52024E025C3DF34C17E974EB4F88\sketch\petitcat\_arduino.ino.cpp -o nul

Alternatives for WiFiEsp.h: [WiFiEsp@2.2.2]

ResolveLibrary(WiFiEsp.h)

-> candidates: [WiFiEsp@2.2.2]

C:\Users\howar\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7/bin/avr-g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -flto -w -x c++ -E -CC -mmcu=atmega328p -DF\_CPU=16000000L -DARDUINO=10607 -DARDUINO\_AVR\_UNO -DARDUINO\_ARCH\_AVR -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\cores\arduino -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\variants\standard -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino\_JSON\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\WiFiEsp\src C:\Users\howar\AppData\Local\Temp\arduino\sketches\F46E52024E025C3DF34C17E974EB4F88\sketch\petitcat\_arduino.ino.cpp -o nul

Alternatives for Adafruit\_TCS34725.h: [Adafruit TCS34725@1.4.4]

ResolveLibrary(Adafruit\_TCS34725.h)

-> candidates: [Adafruit TCS34725@1.4.4]

C:\Users\howar\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7/bin/avr-g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -flto -w -x c++ -E -CC -mmcu=atmega328p -DF\_CPU=16000000L -DARDUINO=10607 -DARDUINO\_AVR\_UNO -DARDUINO\_ARCH\_AVR -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\cores\arduino -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\variants\standard -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino\_JSON\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\WiFiEsp\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_TCS34725 C:\Users\howar\AppData\Local\Temp\arduino\sketches\F46E52024E025C3DF34C17E974EB4F88\sketch\petitcat\_arduino.ino.cpp -o nul

Alternatives for Adafruit\_I2CDevice.h: [Adafruit BusIO@1.15.0]

ResolveLibrary(Adafruit\_I2CDevice.h)

-> candidates: [Adafruit BusIO@1.15.0]

C:\Users\howar\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7/bin/avr-g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -flto -w -x c++ -E -CC -mmcu=atmega328p -DF\_CPU=16000000L -DARDUINO=10607 -DARDUINO\_AVR\_UNO -DARDUINO\_ARCH\_AVR -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\cores\arduino -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\variants\standard -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino\_JSON\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\WiFiEsp\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_TCS34725 -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_BusIO C:\Users\howar\AppData\Local\Temp\arduino\sketches\F46E52024E025C3DF34C17E974EB4F88\sketch\petitcat\_arduino.ino.cpp -o nul

Alternatives for Wire.h: [Wire@1.0]

ResolveLibrary(Wire.h)

-> candidates: [Wire@1.0]

C:\Users\howar\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7/bin/avr-g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -flto -w -x c++ -E -CC -mmcu=atmega328p -DF\_CPU=16000000L -DARDUINO=10607 -DARDUINO\_AVR\_UNO -DARDUINO\_ARCH\_AVR -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\cores\arduino -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\variants\standard -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino\_JSON\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\WiFiEsp\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_TCS34725 -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_BusIO -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\libraries\Wire\src C:\Users\howar\AppData\Local\Temp\arduino\sketches\F46E52024E025C3DF34C17E974EB4F88\sketch\petitcat\_arduino.ino.cpp -o nul

Alternatives for Servo.h: [Servo@1.2.1]

ResolveLibrary(Servo.h)

-> candidates: [Servo@1.2.1]

C:\Users\howar\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7/bin/avr-g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -flto -w -x c++ -E -CC -mmcu=atmega328p -DF\_CPU=16000000L -DARDUINO=10607 -DARDUINO\_AVR\_UNO -DARDUINO\_ARCH\_AVR -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\cores\arduino -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\variants\standard -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino\_JSON\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\WiFiEsp\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_TCS34725 -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_BusIO -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\libraries\Wire\src -IC:\Users\howar\AppData\Local\Arduino15\libraries\Servo\src C:\Users\howar\AppData\Local\Temp\arduino\sketches\F46E52024E025C3DF34C17E974EB4F88\sketch\petitcat\_arduino.ino.cpp -o nul

Alternatives for HMC5883L.h: [Arduino-HMC5883L-dev]

ResolveLibrary(HMC5883L.h)

-> candidates: [Arduino-HMC5883L-dev]

C:\Users\howar\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7/bin/avr-g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -flto -w -x c++ -E -CC -mmcu=atmega328p -DF\_CPU=16000000L -DARDUINO=10607 -DARDUINO\_AVR\_UNO -DARDUINO\_ARCH\_AVR -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\cores\arduino -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\variants\standard -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino\_JSON\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\WiFiEsp\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_TCS34725 -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_BusIO -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\libraries\Wire\src -IC:\Users\howar\AppData\Local\Arduino15\libraries\Servo\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino-HMC5883L-dev C:\Users\howar\AppData\Local\Temp\arduino\sketches\F46E52024E025C3DF34C17E974EB4F88\sketch\petitcat\_arduino.ino.cpp -o nul

C:\Users\howar\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7/bin/avr-g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -flto -w -x c++ -E -CC -mmcu=atmega328p -DF\_CPU=16000000L -DARDUINO=10607 -DARDUINO\_AVR\_UNO -DARDUINO\_ARCH\_AVR -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\cores\arduino -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\variants\standard -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino\_JSON\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\WiFiEsp\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_TCS34725 -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_BusIO -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\libraries\Wire\src -IC:\Users\howar\AppData\Local\Arduino15\libraries\Servo\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino-HMC5883L-dev C:\Users\howar\AppData\Local\Temp\arduino\sketches\F46E52024E025C3DF34C17E974EB4F88\sketch\Color.cpp -o nul

C:\Users\howar\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7/bin/avr-g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -flto -w -x c++ -E -CC -mmcu=atmega328p -DF\_CPU=16000000L -DARDUINO=10607 -DARDUINO\_AVR\_UNO -DARDUINO\_ARCH\_AVR -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\cores\arduino -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\variants\standard -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino\_JSON\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\WiFiEsp\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_TCS34725 -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_BusIO -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\libraries\Wire\src -IC:\Users\howar\AppData\Local\Arduino15\libraries\Servo\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino-HMC5883L-dev C:\Users\howar\AppData\Local\Temp\arduino\sketches\F46E52024E025C3DF34C17E974EB4F88\sketch\Floor.cpp -o nul

C:\Users\howar\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7/bin/avr-g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -flto -w -x c++ -E -CC -mmcu=atmega328p -DF\_CPU=16000000L -DARDUINO=10607 -DARDUINO\_AVR\_UNO -DARDUINO\_ARCH\_AVR -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\cores\arduino -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\variants\standard -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino\_JSON\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\WiFiEsp\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_TCS34725 -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_BusIO -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\libraries\Wire\src -IC:\Users\howar\AppData\Local\Arduino15\libraries\Servo\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino-HMC5883L-dev C:\Users\howar\AppData\Local\Temp\arduino\sketches\F46E52024E025C3DF34C17E974EB4F88\sketch\Head.cpp -o nul

C:\Users\howar\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7/bin/avr-g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -flto -w -x c++ -E -CC -mmcu=atmega328p -DF\_CPU=16000000L -DARDUINO=10607 -DARDUINO\_AVR\_UNO -DARDUINO\_ARCH\_AVR -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\cores\arduino -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\variants\standard -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino\_JSON\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\WiFiEsp\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_TCS34725 -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_BusIO -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\libraries\Wire\src -IC:\Users\howar\AppData\Local\Arduino15\libraries\Servo\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino-HMC5883L-dev C:\Users\howar\AppData\Local\Temp\arduino\sketches\F46E52024E025C3DF34C17E974EB4F88\sketch\Imu.cpp -o nul

C:\Users\howar\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7/bin/avr-g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -flto -w -x c++ -E -CC -mmcu=atmega328p -DF\_CPU=16000000L -DARDUINO=10607 -DARDUINO\_AVR\_UNO -DARDUINO\_ARCH\_AVR -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\cores\arduino -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\variants\standard -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino\_JSON\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\WiFiEsp\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_TCS34725 -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_BusIO -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\libraries\Wire\src -IC:\Users\howar\AppData\Local\Arduino15\libraries\Servo\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino-HMC5883L-dev C:\Users\howar\AppData\Local\Temp\arduino\sketches\F46E52024E025C3DF34C17E974EB4F88\sketch\Interaction.cpp -o nul

C:\Users\howar\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7/bin/avr-g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -flto -w -x c++ -E -CC -mmcu=atmega328p -DF\_CPU=16000000L -DARDUINO=10607 -DARDUINO\_AVR\_UNO -DARDUINO\_ARCH\_AVR -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\cores\arduino -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\variants\standard -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino\_JSON\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\WiFiEsp\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_TCS34725 -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_BusIO -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\libraries\Wire\src -IC:\Users\howar\AppData\Local\Arduino15\libraries\Servo\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino-HMC5883L-dev C:\Users\howar\AppData\Local\Temp\arduino\sketches\F46E52024E025C3DF34C17E974EB4F88\sketch\Led.cpp -o nul

C:\Users\howar\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7/bin/avr-g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -flto -w -x c++ -E -CC -mmcu=atmega328p -DF\_CPU=16000000L -DARDUINO=10607 -DARDUINO\_AVR\_UNO -DARDUINO\_ARCH\_AVR -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\cores\arduino -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\variants\standard -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino\_JSON\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\WiFiEsp\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_TCS34725 -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_BusIO -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\libraries\Wire\src -IC:\Users\howar\AppData\Local\Arduino15\libraries\Servo\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino-HMC5883L-dev C:\Users\howar\AppData\Local\Temp\arduino\sketches\F46E52024E025C3DF34C17E974EB4F88\sketch\Sequencer.cpp -o nul

C:\Users\howar\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7/bin/avr-g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -flto -w -x c++ -E -CC -mmcu=atmega328p -DF\_CPU=16000000L -DARDUINO=10607 -DARDUINO\_AVR\_UNO -DARDUINO\_ARCH\_AVR -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\cores\arduino -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\variants\standard -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino\_JSON\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\WiFiEsp\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_TCS34725 -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_BusIO -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\libraries\Wire\src -IC:\Users\howar\AppData\Local\Arduino15\libraries\Servo\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino-HMC5883L-dev C:\Users\howar\AppData\Local\Temp\arduino\sketches\F46E52024E025C3DF34C17E974EB4F88\sketch\Wheel.cpp -o nul

C:\Users\howar\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7/bin/avr-g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -flto -w -x c++ -E -CC -mmcu=atmega328p -DF\_CPU=16000000L -DARDUINO=10607 -DARDUINO\_AVR\_UNO -DARDUINO\_ARCH\_AVR -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\cores\arduino -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\variants\standard -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino\_JSON\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\WiFiEsp\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_TCS34725 -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_BusIO -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\libraries\Wire\src -IC:\Users\howar\AppData\Local\Arduino15\libraries\Servo\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino-HMC5883L-dev C:\Users\howar\AppData\Local\Temp\arduino\sketches\F46E52024E025C3DF34C17E974EB4F88\sketch\src\interactions\Backward.cpp -o nul

C:\Users\howar\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7/bin/avr-g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -flto -w -x c++ -E -CC -mmcu=atmega328p -DF\_CPU=16000000L -DARDUINO=10607 -DARDUINO\_AVR\_UNO -DARDUINO\_ARCH\_AVR -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\cores\arduino -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\variants\standard -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino\_JSON\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\WiFiEsp\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_TCS34725 -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_BusIO -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\libraries\Wire\src -IC:\Users\howar\AppData\Local\Arduino15\libraries\Servo\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino-HMC5883L-dev C:\Users\howar\AppData\Local\Temp\arduino\sketches\F46E52024E025C3DF34C17E974EB4F88\sketch\src\interactions\Circumvent.cpp -o nul

C:\Users\howar\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7/bin/avr-g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -flto -w -x c++ -E -CC -mmcu=atmega328p -DF\_CPU=16000000L -DARDUINO=10607 -DARDUINO\_AVR\_UNO -DARDUINO\_ARCH\_AVR -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\cores\arduino -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\variants\standard -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino\_JSON\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\WiFiEsp\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_TCS34725 -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_BusIO -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\libraries\Wire\src -IC:\Users\howar\AppData\Local\Arduino15\libraries\Servo\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino-HMC5883L-dev C:\Users\howar\AppData\Local\Temp\arduino\sketches\F46E52024E025C3DF34C17E974EB4F88\sketch\src\interactions\Forward.cpp -o nul

C:\Users\howar\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7/bin/avr-g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -flto -w -x c++ -E -CC -mmcu=atmega328p -DF\_CPU=16000000L -DARDUINO=10607 -DARDUINO\_AVR\_UNO -DARDUINO\_ARCH\_AVR -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\cores\arduino -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\variants\standard -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino\_JSON\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\WiFiEsp\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_TCS34725 -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_BusIO -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\libraries\Wire\src -IC:\Users\howar\AppData\Local\Arduino15\libraries\Servo\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino-HMC5883L-dev C:\Users\howar\AppData\Local\Temp\arduino\sketches\F46E52024E025C3DF34C17E974EB4F88\sketch\src\interactions\Scan.cpp -o nul

C:\Users\howar\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7/bin/avr-g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -flto -w -x c++ -E -CC -mmcu=atmega328p -DF\_CPU=16000000L -DARDUINO=10607 -DARDUINO\_AVR\_UNO -DARDUINO\_ARCH\_AVR -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\cores\arduino -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\variants\standard -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino\_JSON\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\WiFiEsp\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_TCS34725 -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_BusIO -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\libraries\Wire\src -IC:\Users\howar\AppData\Local\Arduino15\libraries\Servo\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino-HMC5883L-dev C:\Users\howar\AppData\Local\Temp\arduino\sketches\F46E52024E025C3DF34C17E974EB4F88\sketch\src\interactions\Swipe.cpp -o nul

C:\Users\howar\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7/bin/avr-g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -flto -w -x c++ -E -CC -mmcu=atmega328p -DF\_CPU=16000000L -DARDUINO=10607 -DARDUINO\_AVR\_UNO -DARDUINO\_ARCH\_AVR -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\cores\arduino -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\variants\standard -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino\_JSON\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\WiFiEsp\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_TCS34725 -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_BusIO -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\libraries\Wire\src -IC:\Users\howar\AppData\Local\Arduino15\libraries\Servo\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino-HMC5883L-dev C:\Users\howar\AppData\Local\Temp\arduino\sketches\F46E52024E025C3DF34C17E974EB4F88\sketch\src\interactions\Turn.cpp -o nul

C:\Users\howar\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7/bin/avr-g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -flto -w -x c++ -E -CC -mmcu=atmega328p -DF\_CPU=16000000L -DARDUINO=10607 -DARDUINO\_AVR\_UNO -DARDUINO\_ARCH\_AVR -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\cores\arduino -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\variants\standard -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino\_JSON\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\WiFiEsp\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_TCS34725 -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_BusIO -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\libraries\Wire\src -IC:\Users\howar\AppData\Local\Arduino15\libraries\Servo\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino-HMC5883L-dev C:\Users\howar\AppData\Local\Temp\arduino\sketches\F46E52024E025C3DF34C17E974EB4F88\sketch\src\interactions\Turn\_head.cpp -o nul

C:\Users\howar\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7/bin/avr-g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -flto -w -x c++ -E -CC -mmcu=atmega328p -DF\_CPU=16000000L -DARDUINO=10607 -DARDUINO\_AVR\_UNO -DARDUINO\_ARCH\_AVR -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\cores\arduino -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\variants\standard -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino\_JSON\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\WiFiEsp\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_TCS34725 -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_BusIO -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\libraries\Wire\src -IC:\Users\howar\AppData\Local\Arduino15\libraries\Servo\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino-HMC5883L-dev C:\Users\howar\AppData\Local\Temp\arduino\sketches\F46E52024E025C3DF34C17E974EB4F88\sketch\src\interactions\Watch.cpp -o nul

C:\Users\howar\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7/bin/avr-g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -flto -w -x c++ -E -CC -mmcu=atmega328p -DF\_CPU=16000000L -DARDUINO=10607 -DARDUINO\_AVR\_UNO -DARDUINO\_ARCH\_AVR -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\cores\arduino -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\variants\standard -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino\_JSON\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\WiFiEsp\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_TCS34725 -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_BusIO -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\libraries\Wire\src -IC:\Users\howar\AppData\Local\Arduino15\libraries\Servo\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino-HMC5883L-dev C:\Users\howar\AppData\Local\Temp\arduino\sketches\F46E52024E025C3DF34C17E974EB4F88\sketch\src\lib\MMC5883.cpp -o nul

C:\Users\howar\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7/bin/avr-g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -flto -w -x c++ -E -CC -mmcu=atmega328p -DF\_CPU=16000000L -DARDUINO=10607 -DARDUINO\_AVR\_UNO -DARDUINO\_ARCH\_AVR -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\cores\arduino -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\variants\standard -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino\_JSON\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\WiFiEsp\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_TCS34725 -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_BusIO -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\libraries\Wire\src -IC:\Users\howar\AppData\Local\Arduino15\libraries\Servo\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino-HMC5883L-dev C:\Users\howar\AppData\Local\Temp\arduino\sketches\F46E52024E025C3DF34C17E974EB4F88\sketch\src\lib\MPU6050.cpp -o nul

C:\Users\howar\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7/bin/avr-g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -flto -w -x c++ -E -CC -mmcu=atmega328p -DF\_CPU=16000000L -DARDUINO=10607 -DARDUINO\_AVR\_UNO -DARDUINO\_ARCH\_AVR -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\cores\arduino -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\variants\standard -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino\_JSON\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\WiFiEsp\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_TCS34725 -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Adafruit\_BusIO -IC:\Users\howar\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.6\libraries\Wire\src -IC:\Users\howar\AppData\Local\Arduino15\libraries\Servo\src -IC:\Users\howar\OneDrive\Documents\Arduino\libraries\Arduino-HMC5883L-dev C:\Users\howar\AppData\Local\Temp\arduino\sketches\F46E52024E025C3DF34C17E974EB4F88\sketch\src\wifi\WifiCat.cpp -o nul

Alternatives for arduino\_secrets.h: []

ResolveLibrary(arduino\_secrets.h)

-> candidates: []

C:\Users\howar\OneDrive\Documents\Arduino\osoyoo\petitcat\_arduino\src\wifi\WifiCat.cpp:11:10: fatal error: arduino\_secrets.h: No such file or directory

#include "arduino\_secrets.h"

^~~~~~~~~~~~~~~~~~~

compilation terminated.

exit status 1

Compilation error: arduino\_secrets.h: No such file or directory